Figure 3. Temperature at 39-m depth for the radiator patterns of the large-scale CTD/ADCP surveys at the tidal mixing front (TMF). Hydrographic properties obtained by averaging SeaSoar data over four minutes (0.85 km horizontally) and by 2-db vertically (averaged data locations indicated by white dots). Mooring locations indicated by black plus signs.