breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
2 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
7 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
8 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
9 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
10 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
11 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
12 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
14 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
T/STD nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
