# NAVIGATION FROM TT007NAV.___-___ ADCP:PINGDATA.000-.000
# 15 minute interruption of cast due to current trip condition
# "approximately 89% of flow through filters at depths indicated
# all times are given as local time (Z time -10 hrs)
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
2 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
7 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
8 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
9 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
10 70 66 MAY E 7 3806.6 1532.9 x nd nd nd nd x nd 0.6591 0.2654 nd nd nd nd nd 
11 167 157 JULY* G 9 5080.6 1338.0 x nd nd nd nd x nd 0.8798 0.2317 nd nd nd nd nd 
12 264 248 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 362 340 AUG H 10 5674.9 1336.1 x nd nd nd nd x x 0.9827 0.2314 nd nd nd nd nd 
14 459 431 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 557 523 SEP I 11 5647.2 1398.6 x nd nd nd nd x nd 0.9779 0.2422 nd nd nd nd nd 
T/STD 602 565 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
