# NAVIGATION FROM TT007NAV.___-___ ADCP:PINGDATA.158-167
# all times are given as local time (Z time -10 hrs)
# nominal depths are corrected to actual depth by pressure transducer data
# The station began with 1h:20min needed for respooling wire to 550 m and back.
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 49 48 JAN I 36 6311.0 3013.2 x nd nd nd nd x x 0.390 0.186 0.0135 0.0098 0.0136 0.0249 1.8235 
2 73 71 APR* H 35 6506.0 2928.0 x 3 4 1.2a 1.2b x nd 0.402 0.181 0.0211 0.0166 0.0210 0.0379 1.8101 
7 144 140 FEB G 34 11222.6 2859.9 x nd nd nd nd x x 0.693 0.177 0.0160 0.0130 0.0162 0.0254 1.5684 
8 192 187 MAR F 33 12150.0 2791.7 x nd nd nd nd x nd 0.750 0.172 0.0123 0.0104 0.0122 0.0186 1.5208 
9 290 282 MAY E 32 12498.3 2735.0 x nd nd nd nd x x 0.771 0.169 0.0098 0.0083 0.0098 0.0149 1.5242 
10 389 379 JULY* D 31 11511.8 2666.8 x nd nd nd nd x nd 0.711 0.165 0.0102 0.0086 0.0102 0.0151 1.4813 
11 486 473 AUG C 30 12906.3 2613.8 x nd nd nd nd x x 0.797 0.161 0.0089 0.0072 0.0091 0.0134 1.4761 
12 583 568 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 681 663 OCT B 29 12736.0 2797.4 x nd nd nd nd x nd 0.786 0.173 0.0070 0.0056 0.0072 0.0102 1.4173 
14 778 757 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 876 853 NOV A 28 12879.6 2574.1 x nd nd nd nd x x 0.795 0.159 0.0063 0.0052 0.0063 0.0090 1.4113 
T/STD 921 897 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
