# NAVIGATION FROM TT007NAV.___-___ ADCP:PINGDATA.187-194
# Limited time necessitated only 3hrs of operation.
# the correct direction of motor rotiation is clockwise
# nominal depths are corrected data from pump April and end of wire STD.
# (B) in subsample listing: Bidigare got large punch: Hedges mq sample was with sm
# Wheeler's samples look fine.
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
2 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
7 32 32 JAN J 24 4486.8 1943.8 x nd nd nd nd B nd 0.415 0.180 0.0142 0.0089 0.0151 0.0283 1.8817 
8 80 80 APR* D 40 4842.7 1934.3 x 5 6 1.5 1.5 xB x 0.448 0.179 0.0154 0.0097 0.0162 0.0288 1.7783 
9 178 178 FEB A 37 8930.5 1803.7 x nd nd nd nd nd x 0.827 0.167 0.0113 0.0085 0.0117 0.0174 1.4833 
10 277 277 MAR C 39 9064.1 1807.5 x nd nd nd nd nd nd 0.839 0.167 0.0111 0.0086 0.0114 0.0167 1.4709 
11 374 374 MAY E 41 9314.0 1739.4 x 7 8 1.6 1.6 nd nd 0.862 0.161 0.0082 0.0066 0.0083 0.0123 1.4685 
12 471 472 JULY* B 38 8373.3 1711.0 x nd nd nd nd nd nd 0.775 0.158 0.0081 0.0061 0.0084 0.0127 nd 
13 569 570 AUG F 42 9264.0 1699.6 x 9 10 1.3 1.3 nd nd 0.858 0.157 0.0052 0.0040 0.0054 0.0078 1.4498 
14 666 667 OCT G 43 9249.6 1775.4 x nd nd nd nd nd nd 0.856 0.164 0.0045 0.0030 0.0048 0.0072 nd 
15 764 765 NOV H 44 9259.7 1603.1 x 11 12 1.4 1.4 nd nd 0.857 0.148 0.0041 0.0030 0.0042 0.0063 1.5221 
T/STD 809 810 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
