# NAVIGATION FROM: TT007NAV.___-____  ADCP:PINGDATA.260-267.
# Raining hard during deployment and recovery.
# the correct direction of motor rotiation is clockwise
# nominal depths are corrected using data from pump April and end of wire STD.
# all times are given as local time (Z time -10 hrs)
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 19 19 JAN A 55 7141.5 3011.3 x nd nd nd nd x x 0.397 0.167 0.0139 0.0088 0.0148 0.0260 1.9376 
2 43 42 MAY B 56 7170.9 3052.9 x 23 24 '1.12 '1.12 x nd 0.398 0.170 0.0143 0.0088 0.0139 0.0264 1.8569 
7 114 112 FEB C 57 9968.5 3066.2 x nd nd nd nd x x 0.554 0.170 0.0143 0.0109 0.0143 0.0243 1.6936 
8 162 159 MAR D 58 11851.3 3035.9 x w2.1 w2.1 2.2 2.2 x nd 0.658 0.169 0.0140 0.0117 0.0140 0.0223 1.5903 
9 260 255 JUL F 60 11762.8 2823.9 x nd nd nd nd x x 0.653 0.157 0.0144 0.0116 0.0146 0.0225 1.5006 
10 359 353 APR* G 61 12845.4 2964.0 x 29 30 2.5 2.5 x nd 0.714 0.165 0.0139 0.0120 0.0138 0.0207 1.4384 
11 456 448 AUG E 59 13877.7 2763.3 x 25 26 2.3 2.3 x x 0.771 0.154 0.0092 0.0076 0.0091 0.0135 1.4066 
12 553 543 nd nd nd nd nd x nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 651 640 OCT H 62 13803.8 2911.0 x nd nd nd nd x nd 0.767 0.162 0.0058 0.0043 0.0057 0.0085 1.4144 
14 748 735 nd nd nd nd nd x nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 846 831 NOV I 63 14389.4 2608.1 x 27 28 2.4 2.4 x x 0.799 0.145 0.0053 0.0033 0.0056 0.0080 1.4857 
T/STD 891 875 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
