# NAVIGATION FROM: TT007NAV.131-136  ADCP:PINGDATA.300-308
# Delayed start due to respooling cable to 600m and back
# April one Wheeler filter detatched but no evidence from flow record of problem.
# Oct shaken coming off wire
# Repaired wet splice above term #9 prior to cast
# nominal depths are corrected using data from pump April and end of wire STD.
# all times are given as local time (Z time -10 hrs)
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 15 15 JAN A 64 6719.5 2943.1 x nd nd nd nd x x 0.373 0.164 0.0165 0.0113 0.0168 0.0334 1.9376 
2 39 39 MAY B 65 7508.7 2984.8 x w31 32 2.7 2.7 x nd 0.417 0.166 0.0181 0.0139 0.0181 0.0334 1.8569 
7 110 111 FEB C 66 12181.4 2886.4 x nd nd nd nd x x 0.677 0.160 0.0090 0.0075 0.0088 0.0150 1.6936 
8 158 159 MAR D 67 13292.1 2962.1 x nd nd 2.6 2.6 x nd 0.738 0.165 0.0097 0.0080 0.0098 0.0149 1.5903 
9 256 258 AUG E 68 13110.4 2808.8 x w33 34 2.8 2.8 x x 0.728 0.156 0.0126 0.0110 0.0124 0.0191 1.5006 
10 355 358 JUL F 69 12307.1 2789.8 x nd nd nd nd x nd 0.684 0.155 0.0117 0.0096 0.0118 0.0177 1.4384 
11 452 455 APR* G 70 13806.9 2823.9 x w35 36 2.9 2.9b x x 0.767 0.157 0.0090 0.0079 0.0089 0.0131 1.4066 
12 549 553 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 647 652 OCT H 71 13423.4 2939.4 x nd nd nd nd x nd 0.746 0.163 0.0084 0.0073 0.0083 0.0119 1.4144 
14 744 749 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 842 848 NOV I 72 14312.2 2678.2 x w37 38 '2.10 '2.10 x x 0.795 0.149 0.0047 0.0040 0.0046 0.0070 1.4857 
T/STD 887 893 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
