# NAVIGATION FROM: TT007NAV.187-191  ADCP:PINGDATA.383-391
# Stormy during deployment. Deepest with wire 20deg aft
# nominal depths are corrected using data from pump April and end of wire STD.
# all times are given as local time (Z time -10 hrs)
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 25 24 JAN A 83 6439.3 1970.3 x nd nd nd nd x x 0.358 0.109 0.0159 0.0107 0.0162 0.0322 1.9376 
2 49 48 MAY B 84 6845.9 2797.4 x w50 51 3.4 3.4 xB nd 0.380 0.155 0.0140 0.0099 0.0140 0.0287 1.8569 
7 120 117 FEB C 85 9294.7 2729.3 x nd nd nd nd x x 0.516 0.152 0.0143 0.0114 0.0143 0.0245 1.6936 
8 168 163 MAR D 86 11860.4 2861.8 x nd nd 3.5 3.5 x nd 0.659 0.159 0.0147 0.0121 0.0146 0.0244 1.5903 
9 266 258 JUL E 87 12624.3 2591.1 x nd nd nd nd x x 0.701 0.144 0.0095 0.0081 0.0094 0.0143 1.5006 
10 365 355 AUG F 88 14004.5 2534.3 x w52 53 3.6 3.6 x nd 0.778 0.141 0.0080 0.0062 0.0081 0.0120 1.4384 
11 462 449 OCT G 89 13535.5 2700.9 x nd nd nd nd x x 0.752 0.150 0.0068 0.0058 0.0068 0.0099 1.4066 
12 559 543 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 657 638 NOV H 90 13774.3 2572.2 x w54 55 3.7 3.7 x nd 0.765 0.143 0.0058 0.0048 0.0059 0.0087 1.4144 
14 754 732 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 852 828 APR* I 91 14462.5 2600.6 x w56 57 3.8 3.8 x x 0.803 0.144 0.0039 0.0033 0.0039 0.0060 1.4857 
T/STD 897 871 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
