# NAVIGATION FROM: TT007NAV.207-211  ADCP:PINGDATA.409-416
# Filter holder B check valve may be no good.
# Quiescent during deployment. low currents.
# nominal depths are corrected to actual depth by pressure transducer data from pu
# all times are given as local time (Z time -10 hrs)
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 20 20 JAN A 92 5039.3 2485.1 x nd nd nd nd x x 0.295 0.145 0.0148 0.0093 0.0148 0.0339 1.9376 
2 44 44 MAY B 93 5492.0 2579.8 x nd nd nd nd xB nd 0.321 0.151 0.0139 0.0078 0.0144 0.0320 1.8569 
7 115 115 FEB C 94 9186.0 2697.1 x nd nd nd nd x x 0.537 0.158 0.0117 0.0086 0.0120 0.0208 1.6936 
8 163 163 MAR D 95 12324.3 2613.8 x nd nd nd nd x nd 0.721 0.153 0.0092 0.0070 0.0094 0.0153 1.5903 
9 261 261 JUL E 96 11754.0 2487.0 x nd nd nd nd x x 0.687 0.145 0.0067 0.0054 0.0067 0.0105 1.5006 
10 360 360 AUG F 97 13308.9 2488.9 x nd nd nd nd x nd 0.778 0.146 0.0050 0.0035 0.0052 0.0082 1.4384 
11 457 456 OCT G 98 13269.2 2543.8 x nd nd nd nd x x 0.776 0.149 0.0048 0.0038 0.0049 0.0074 1.4066 
12 554 553 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
13 652 651 APR* H 99 13688.6 2477.5 x nd nd nd nd x nd 0.801 0.145 0.0033 0.0028 0.0033 0.0049 1.4144 
14 749 748 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
15 847 846 NOV I 100 13815.0 2411.3 x nd nd nd nd x x 0.808 0.141 0.0031 0.0022 0.0032 0.0049 1.4857 
T/STD 892 891 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
