# NAVIGATION FROM: TT007NAV.251-255  ADCP:PINGDATA.463-470
# (#) JUNE NOT DEPLOYED AS DIPPED BLANK.
# Quiescent during deployment. low currents.
# nominal depths are corrected using data from pump April and end of wire STD.
# all times are given as local time (Z time -10 hrs)
# small punch to Bidigare e101
breakout nom_depth depth pump_id holder_id sample_no l_filtered l_adsorbed ss_ku ss_alt1 ss_alt2 ss_whlr1 ss_whlr2 ss_org1-53 ss_org_gt53 filter_flowrate adsorber_flowrate gt53um_grey_od gt53um_red_od gt53um_green_od gt53um_blue_od blue/green_ratio 
1 15 15 SEPT A 102 4999.0 2888.3 x nd nd nd nd x x 0.292 0.169 0.0058 0.0031 0.0061 0.0116 1.9049 
2 39 39 MAY J 101 5083.4 2670.6 x 58 w59 3.9 3.9 xB nd 0.297 0.156 0.0055 0.0036 0.0054 0.0117 2.1564 
7 110 109 JAN C 103 7868.3 2538.1 x nd nd nd nd x x 0.460 0.148 0.0138 0.0109 0.0139 0.0226 1.6310 
8 158 157 MAR D 104 11752.2 2661.1 x nd nd '3.10 '3.10 x nd 0.687 0.156 0.0082 0.0066 0.0084 0.0121 1.4403 
9 256 255 FEB E 105 14243.5 2494.6 x nd nd nd nd x x 0.833 0.146 0.0064 0.0048 0.0067 0.0094 1.4107 
10 355 353 JUL F 106 12482.5 2333.7 x '3.11 '3.11 '3.12 '3.12 x nd 0.730 0.136 0.0054 0.0042 0.0056 0.0077 1.3636 
11 452 450 AUG G 107 13783.4 2369.7 x nd nd nd nd x x 0.806 0.139 0.0040 0.0030 0.0041 0.0061 1.4615 
12 549 546 OCT H 108 13647.1 2545.7 x nd nd nd nd x nd 0.798 0.149 0.0036 0.0027 0.0037 0.0053 nd 
13 647 643 APR* I 109 14000.3 2464.3 x 60 w61 4.1 4.1 x x 0.819 0.144 0.0030 0.0021 0.0031 0.0045 1.4286 
14 744 740 JUNE# B 110 nd nd nd nd nd nd nd x x nd nd nd nd nd nd nd 
15 842 837 NOV M 111 13578.6 2364.0 x 62 w63 4.2 4.2 x nd 0.794 0.138 0.0021 0.0015 0.0021 0.0032 1.4896 
T/STD 887 882 nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd nd 
